\hypertarget{structel_bluetooth_lego_nxt}{}\section{el\+Bluetooth\+Lego\+Nxt Struct Reference}
\label{structel_bluetooth_lego_nxt}\index{el\+Bluetooth\+Lego\+Nxt@{el\+Bluetooth\+Lego\+Nxt}}
\subsection*{Public Attributes}
\begin{DoxyCompactItemize}
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_af9b86753894a66f0fe16ebea23a8e8fb}\label{structel_bluetooth_lego_nxt_af9b86753894a66f0fe16ebea23a8e8fb}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Bluetooth\+Init} )(E\+L\+U\+Int32 portid)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_a200b3ecc4faaf4c00fc7768ee49971fc}\label{structel_bluetooth_lego_nxt_a200b3ecc4faaf4c00fc7768ee49971fc}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Initialize\+Master} )(E\+L\+U\+Int32 portid, const E\+L\+U\+Char $\ast$addr, const E\+L\+Char $\ast$p\+Pin)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_a01649b06b7ca55d613786a27da461297}\label{structel_bluetooth_lego_nxt_a01649b06b7ca55d613786a27da461297}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Initialize\+Slave} )(E\+L\+U\+Int32 portid, const E\+L\+Char $\ast$p\+Pin)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_aceb75783fb6f4b4311763f839823d045}\label{structel_bluetooth_lego_nxt_aceb75783fb6f4b4311763f839823d045}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Terminate} )(E\+L\+U\+Int32 portid)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_af78fe4c646dd7f13b9a79475cfac18ff}\label{structel_bluetooth_lego_nxt_af78fe4c646dd7f13b9a79475cfac18ff}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Send\+Data} )(E\+L\+U\+Int32 portid, const E\+L\+U\+Int8 $\ast$buf, E\+L\+U\+Int32 offset, E\+L\+U\+Int32 len, E\+L\+U\+Int32 $\ast$outsize)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_af80d4d01d535b7b3c409de1ecf37bd43}\label{structel_bluetooth_lego_nxt_af80d4d01d535b7b3c409de1ecf37bd43}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Receive\+Data} )(E\+L\+U\+Int32 portid, E\+L\+U\+Int8 $\ast$buf, E\+L\+U\+Int32 offset, E\+L\+U\+Int32 len, E\+L\+U\+Int32 $\ast$outsize)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_af8e70f65bb9059941467a0360278554b}\label{structel_bluetooth_lego_nxt_af8e70f65bb9059941467a0360278554b}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Get\+Device\+Name} )(E\+L\+U\+Int32 portid, E\+L\+Char $\ast$p\+Name)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_a4fb67d73943d2ce65bdf2e376ef9233e}\label{structel_bluetooth_lego_nxt_a4fb67d73943d2ce65bdf2e376ef9233e}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Set\+Device\+Name} )(E\+L\+U\+Int32 portid, const E\+L\+Char $\ast$p\+Name)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_a7504bbbc73effb4903b5200484d5166e}\label{structel_bluetooth_lego_nxt_a7504bbbc73effb4903b5200484d5166e}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Get\+Status} )(E\+L\+U\+Int32 portid, E\+L\+Int32 $\ast$p\+Status)
\item 
\mbox{\Hypertarget{structel_bluetooth_lego_nxt_a4a4238988eabf07689138fc7311a6290}\label{structel_bluetooth_lego_nxt_a4a4238988eabf07689138fc7311a6290}} 
E\+L\+Int32($\ast$ {\bfseries p\+Fnc\+Get\+Signal\+Strength} )(E\+L\+U\+Int32 portid, E\+L\+Int32 $\ast$p\+Strength)
\end{DoxyCompactItemize}


The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
/\+Users/nakamura/openel/\+Open\+E\+L-\/3.\+0.\+0/include/\mbox{\hyperlink{open_e_l___n_x_t_8h}{open\+E\+L\+\_\+\+N\+X\+T.\+h}}\end{DoxyCompactItemize}
